* Ductile damage model parameters are obtained from Bayesian optimisation and FE.
* Errors of less than 2%, comparing experimental and simulation data, are reported.
* The automated approach requires minimal user input.